AC MINI CURRENT SWTICH

CS-610-75 Mini Series

The CS-610-75 mini series incorporates:

* auto-ranging
* self-powered and no insertion loss
* true digital switching and no leakage
* field adjustable setpoint
* solid-state reliability
* input / output isolation via current transformer

PRODUCT HIGHLIGHTS

* compact form factor
* solid, reliable mounting

SPECIFICATIONS

|  |  |
| --- | --- |
| SPECIFICATIONS |  |
| CURRENT SETPOINT | Adjustable - 0.75 to 75 Amps |
| MAXIMUM INPUT CURRENT | 75 Amps continuous |
| SENSOR POWER | Self-powered |
| OUTPUT TYPE | Solid-state mosfet |
| OUTPUT SWITCH ACTION | Normally open |
| OUTPUT SWITCH RATINGS | 30 Vac/dc, 500 mA max |
| VON @ 24 VDC AT 500 mA | <50 mV |
| FREQUENCY | 50/60 Hz |
| RESPONSE TIME | 200 mS typical |
| INSULATION CLASS | 600 Vac, insulated conductors |
| OPERATING TEMPERATURE | -15 to 60°C (5 to 140°F) |
| OPERATING HUMIDITY | 5 to 90 %RH non-condensing |
| WIRING CONNECTIONS | Screw terminal block (14 to 22 AWG) |
| DIMENSIONS | 48mm W x 49mm H x 21mm D (1.9” x 1.93” x 0.83”) |
| SENSOR APERTURE | 11.4mm (0.45”) |
| ENCLOSURE MATERIAL AGENCY | ABS/PC, UL94-V0 |
| APPROVALS | cULus listed |