COMMAND RELAY

CSR Series

The CSR-112 and CSR-124 Command Relays are line voltage relays for use with the CS and SC current sensors and switches or as stand-alone devices. All models are UL approved and are CE compliant.

PRODUCT HIGHLIGHTS

* Can be easily mounted to any CS or SC (Except CS Mini)
* Convenient Relay Status LED
* Can be factory assembled
* SPDT Form C relay contacts
* Environmentally-friendly cadmium-free contacts
* Ideal for switching contactors, solenoids and motors
* Small compact size

SPECIFICATIONS

|  |  |
| --- | --- |
| SPECIFICATIONS |  |
| COIL VOLTAGE | **CSR-112:** 12 Vdc ±10%  **CSR-124:** 24 Vac/dc ±10% |
| COIL CURRENT | **CSR-112:** 25 mA maximum  **CSR-124:** 13 mA maximum |
| RELAY CONTACTS | SPDT From C (NO + NC) |
| CONTACT RATINGS | 5A @ 250 Vac/30 Vdc resistive  2A @ 250 Vac/30 Vdc resistive |
| CONTACT RESISTANCE | 30 mΩ maximum |
| OPERATING TEMPERATURE | -15 to 60°C (5 to 140°F) |
| OPERATING HUMIDITY | 5 to 90 %RH, non-condensing |
| WIRING CONNECTION | Terminal block (14 to 22 AWG) |
| DIMENSIONS | 50.8mm W x 35.6mm H x 21.1mm D (2” x 1.4” x 0.83”) |
| ENCLOSURE MATERIAL | ABS/PC, UL94-V0 |
| AGENCY APPROVALS | cULus listed |