OUTSIDE PRESSURE VENT

OPV Series

The single point outside pressure port is used to sample outside air pressure and supply pressure sensor.

PRODUCT HIGHLIGHTS

* Compact form factor enclosure with soft close cover
* IP 65 Enclosure
* Slotted mounting holes angled for ease of field installation
* Custom branding available
* Multiple mounting options
* Available with top or rear wiring access hole
* Barbed fitting for hose connection

SPECIFICATIONS

|  |  |
| --- | --- |
| SPECIFICATIONS |  |
| HOSE FITTING | Barbed fitting, min 3/16” ID tubing |
| AMBIENT OPERATING RANGE | -40 to 50°C (-40 to 122°F), 5 to 95 %RH non-condensing |
| ENCLOSURE | Polycarbonate, UL94-V0, IP65 (NEMA 4X) |
| WIRE ACCESS HOLE | Rear Entry or Top entry hole for conduit or cable gland. 21.83mm (0.859”) diameter. |
| COUNTRY OF ORIGIN | Canada |