AC CURRENT SWTICH

CS-610-200 Series

The CS-610-200 series incorporates:

* auto-ranging
* self-powered and no insertion loss
* true digital switching and no leakage
* field adjustable setpoint
* status and power LED’s
* solid-state reliability
* input / output isolation via current transformer

PRODUCT HIGHLIGHTS

* compact form factor
* solid, reliable mounting
* integrated din rail mounting

SPECIFICATIONS

|  |  |
| --- | --- |
| SPECIFICATIONS |  |
| CURRENT SETPOINT  | Adjustable - 1 to 200 Amps |
| MAXIMUM INPUT CURRENT  | 200 Amps continuous |
| SENSOR POWER  | Self-powered |
| OUTPUT TYPE  | Solid-state mosfet |
| OUTPUT SWITCH ACTION  | Normally open |
| OUTPUT SWITCH RATINGS  | 30 Vac/dc, 500 mA max |
| VON @ 24 VDC AT 500 mA  | <50 mV |
| FREQUENCY  | 50/60 Hz |
| RESPONSE TIME  | 200 mS typical |
| INSULATION CLASS  | 600 Vac, insulated conductors |
| OPERATING TEMPERATURE  | -15 to 50°C (5 to 122°F) |
| OPERATING HUMIDITY  | 5 to 90 %RH non-condensing |
| WIRING CONNECTIONS  | Screw terminal block (14 to 22 AWG) |
| DIMENSIONS  | 67mm W x 68mm H x 24.1mm D (2.65” x 2.7” x 0.95”) |
| SENSOR APERTURE  | 20.3mm (0.8”) |
| ENCLOSURE MATERIAL AGENCY  | ABS/PC, UL94-V0 |
| APPROVALS  | cULus listed |