WATER DETECTOR

WD Series

The WD series incorporates:

* single-point standalone, single-point remote probe or conductivity cable
* fail-safe circuitry
* NO/NC form C, relay output
* weatherproof enclosure

PRODUCT HIGHLIGHTS

* monitors variety of liquids
* alarm on liquid detection, power failure, or internal failure

SPECIFICATIONS

|  |  |
| --- | --- |
| SPECIFICATIONS |  |
| POWER SUPPLY  | 14 - 30 Vac/dc |
| SUPPLY CURRENT  | 60 mA max @ 24 Vdc, (no water) |
| OPERATING TEMPERATURE  | 0 to 70°C (32 to 158°F) |
| CABLE RATING  | Plenum rated - CL2P (UL) |
| ENCLOSURE  | ABS with hinged lid and gasket, UL94-5VB, IP65 (NEMA 4X) |
| DIMENSIONS  | 145mm L x 100mm W x 64mm H (5.7” x 3.95” x 2.5”) |
| HEIGHT WITH MOUNTING  | 98.43mm (3.875”) maximum |
| LEGS (WD100)  | 88.90mm (3.25”) minimum |
| ALARM OUTPUT  | Form C relay, rated @ 2 Amps @ 250 Vac/dc (resistive load) |
| APPROVALS  | CE, RoHS |
| COUNTRY OF ORIGIN  | Canada |