PRESSURE PICKUP PORTS

XPV Series

OPV) OUTSIDE PICK-UP PORT: The OPV is a weatherproof ABS enclosure with an integrated wind shield that incorporates a port with a 3/16” barb fitting for connection of 0.17” ID pneumatic tubing. It can be mounted on the side of a building and used in conjunction with a low pressure transmitter to monitor building pressure.

RPV) STAINLESS STEEL PICK-UP PORT: The RPV is a stainless steel wall plate that incorporates a filtered port with 1/8” barb connection for pneumatic tubing. It can be mounted on a standard junction box or directly to a wall or ceiling and used in conjunction with a low pressure transmitter to monitor room pressure.

CPV) CONTINENTAL ABS PICK-UP PORT: The CPV is a low profile, decorative ABS enclosure that incorporates a port with a 3/16” barb fitting for connection of 0.17” ID pneumatic tubing. It can be mounted on a standard junction box or directly to a wall and used in conjunction with a low pressure transmitter to monitor room pressure.